\hypertarget{coniciap_8h}{
\section{coniciap.h File Reference}
\label{coniciap_8h}\index{coniciap.h@{coniciap.h}}
}


\subsection{Detailed Description}
Con\-Ic\-Iap class. 

Con\-Ic\-Iap class is for access IAPs. 

{\tt \#include $<$glib.h$>$}\par
{\tt \#include $<$glib-object.h$>$}\par
\subsection*{Defines}
\begin{Indent}{\bf Bearers}\par
{\em The bearer types returned by \hyperlink{coniciap_8h_2bf015404731baf91b43f73529db8bcb}{con\_\-ic\_\-iap\_\-get\_\-bearer\_\-type()} and \hyperlink{conicevent_8h_ed4addbb3d49ad41fbd252e33129d8c8}{con\_\-ic\_\-event\_\-get\_\-bearer\_\-type()}.

\begin{Desc}
\item[Note:]More bearer types might be added in the future. \end{Desc}
}\begin{CompactItemize}
\item 
\hypertarget{coniciap_8h_b591cacf72703570e245b62c735c087d}{
\#define \hyperlink{coniciap_8h_b591cacf72703570e245b62c735c087d}{CON\_\-IC\_\-BEARER\_\-WLAN\_\-INFRA}~\char`\"{}WLAN\_\-INFRA\char`\"{}}
\label{coniciap_8h_b591cacf72703570e245b62c735c087d}

\begin{CompactList}\small\item\em WLAN infrastructure mode. \item\end{CompactList}\item 
\hypertarget{coniciap_8h_19bcba94913224615a911a4089aae93a}{
\#define \hyperlink{coniciap_8h_19bcba94913224615a911a4089aae93a}{CON\_\-IC\_\-BEARER\_\-WLAN\_\-ADHOC}~\char`\"{}WLAN\_\-ADHOC\char`\"{}}
\label{coniciap_8h_19bcba94913224615a911a4089aae93a}

\begin{CompactList}\small\item\em WLAN Ad-Hoc mode. \item\end{CompactList}\item 
\hypertarget{coniciap_8h_c2f9e2572816eeb08a297166f9da577c}{
\#define \hyperlink{coniciap_8h_c2f9e2572816eeb08a297166f9da577c}{CON\_\-IC\_\-BEARER\_\-DUN\_\-GSM\_\-CS}~\char`\"{}DUN\_\-GSM\_\-CS\char`\"{}}
\label{coniciap_8h_c2f9e2572816eeb08a297166f9da577c}

\begin{CompactList}\small\item\em Bluetooth Dial-up Networking profile using GSM circuit-switched. \item\end{CompactList}\item 
\hypertarget{coniciap_8h_940cf7a7c5745fc016fdfa0e1c1957e5}{
\#define \hyperlink{coniciap_8h_940cf7a7c5745fc016fdfa0e1c1957e5}{CON\_\-IC\_\-BEARER\_\-DUN\_\-GSM\_\-PS}~\char`\"{}DUN\_\-GSM\_\-PS\char`\"{}}
\label{coniciap_8h_940cf7a7c5745fc016fdfa0e1c1957e5}

\begin{CompactList}\small\item\em Bluetooth Dial-up Networking profile using GSM packet-switched. \item\end{CompactList}\end{CompactItemize}
\end{Indent}
\subsection*{Typedefs}
\begin{CompactItemize}
\item 
typedef \_\-Con\-Ic\-Iap \hyperlink{coniciap_8h_e2a229cb6d3f9b974258522f95ed65d9}{Con\-Ic\-Iap}
\begin{CompactList}\small\item\em Con\-Ic\-Connection\-Event object. \item\end{CompactList}\end{CompactItemize}
\subsection*{Functions}
\begin{CompactItemize}
\item 
const gchar $\ast$ \hyperlink{coniciap_8h_2ac08a9a33db7c11c5d739702429e449}{con\_\-ic\_\-iap\_\-get\_\-name} (\hyperlink{coniciap_8h_e2a229cb6d3f9b974258522f95ed65d9}{Con\-Ic\-Iap} $\ast$iap)
\begin{CompactList}\small\item\em Returns the name of the IAP as string. \item\end{CompactList}\item 
const gchar $\ast$ \hyperlink{coniciap_8h_5a9874e2d03a579acf230bd378c642f8}{con\_\-ic\_\-iap\_\-get\_\-id} (\hyperlink{coniciap_8h_e2a229cb6d3f9b974258522f95ed65d9}{Con\-Ic\-Iap} $\ast$iap)
\begin{CompactList}\small\item\em Returns the ID of the IAP as string. \item\end{CompactList}\item 
const gchar $\ast$ \hyperlink{coniciap_8h_2bf015404731baf91b43f73529db8bcb}{con\_\-ic\_\-iap\_\-get\_\-bearer\_\-type} (\hyperlink{coniciap_8h_e2a229cb6d3f9b974258522f95ed65d9}{Con\-Ic\-Iap} $\ast$iap)
\begin{CompactList}\small\item\em Returns the bearer type of the IAP as string. \item\end{CompactList}\end{CompactItemize}


\subsection{Typedef Documentation}
\hypertarget{coniciap_8h_e2a229cb6d3f9b974258522f95ed65d9}{
\index{coniciap.h@{coniciap.h}!ConIcIap@{ConIcIap}}
\index{ConIcIap@{ConIcIap}!coniciap.h@{coniciap.h}}
\subsubsection[ConIcIap]{\setlength{\rightskip}{0pt plus 5cm}typedef struct \_\-Con\-Ic\-Iap \hyperlink{coniciap_8h_e2a229cb6d3f9b974258522f95ed65d9}{Con\-Ic\-Iap}}}
\label{coniciap_8h_e2a229cb6d3f9b974258522f95ed65d9}


Con\-Ic\-Connection\-Event object. 

The contents of the object is private, to access the object use the functions provided by \hyperlink{conicconnectionevent_8h}{conicconnectionevent.h}. 

\subsection{Function Documentation}
\hypertarget{coniciap_8h_2bf015404731baf91b43f73529db8bcb}{
\index{coniciap.h@{coniciap.h}!con_ic_iap_get_bearer_type@{con\_\-ic\_\-iap\_\-get\_\-bearer\_\-type}}
\index{con_ic_iap_get_bearer_type@{con\_\-ic\_\-iap\_\-get\_\-bearer\_\-type}!coniciap.h@{coniciap.h}}
\subsubsection[con\_\-ic\_\-iap\_\-get\_\-bearer\_\-type]{\setlength{\rightskip}{0pt plus 5cm}const gchar$\ast$ con\_\-ic\_\-iap\_\-get\_\-bearer\_\-type (\hyperlink{coniciap_8h_e2a229cb6d3f9b974258522f95ed65d9}{Con\-Ic\-Iap} $\ast$ {\em iap})}}
\label{coniciap_8h_2bf015404731baf91b43f73529db8bcb}


Returns the bearer type of the IAP as string. 

\begin{Desc}
\item[Parameters:]
\begin{description}
\item[{\em iap}]Con\-Ic\-Iap object \end{description}
\end{Desc}
\begin{Desc}
\item[Returns:]Bearer type of the IAP. \end{Desc}
\hypertarget{coniciap_8h_5a9874e2d03a579acf230bd378c642f8}{
\index{coniciap.h@{coniciap.h}!con_ic_iap_get_id@{con\_\-ic\_\-iap\_\-get\_\-id}}
\index{con_ic_iap_get_id@{con\_\-ic\_\-iap\_\-get\_\-id}!coniciap.h@{coniciap.h}}
\subsubsection[con\_\-ic\_\-iap\_\-get\_\-id]{\setlength{\rightskip}{0pt plus 5cm}const gchar$\ast$ con\_\-ic\_\-iap\_\-get\_\-id (\hyperlink{coniciap_8h_e2a229cb6d3f9b974258522f95ed65d9}{Con\-Ic\-Iap} $\ast$ {\em iap})}}
\label{coniciap_8h_5a9874e2d03a579acf230bd378c642f8}


Returns the ID of the IAP as string. 

\begin{Desc}
\item[Parameters:]
\begin{description}
\item[{\em iap}]Con\-Ic\-Iap object \end{description}
\end{Desc}
\begin{Desc}
\item[Returns:]ID of the IAP. \end{Desc}
\hypertarget{coniciap_8h_2ac08a9a33db7c11c5d739702429e449}{
\index{coniciap.h@{coniciap.h}!con_ic_iap_get_name@{con\_\-ic\_\-iap\_\-get\_\-name}}
\index{con_ic_iap_get_name@{con\_\-ic\_\-iap\_\-get\_\-name}!coniciap.h@{coniciap.h}}
\subsubsection[con\_\-ic\_\-iap\_\-get\_\-name]{\setlength{\rightskip}{0pt plus 5cm}const gchar$\ast$ con\_\-ic\_\-iap\_\-get\_\-name (\hyperlink{coniciap_8h_e2a229cb6d3f9b974258522f95ed65d9}{Con\-Ic\-Iap} $\ast$ {\em iap})}}
\label{coniciap_8h_2ac08a9a33db7c11c5d739702429e449}


Returns the name of the IAP as string. 

\begin{Desc}
\item[Parameters:]
\begin{description}
\item[{\em iap}]Con\-Ic\-Iap object \end{description}
\end{Desc}
\begin{Desc}
\item[Returns:]Name of the IAP. \end{Desc}
